# List of MAC addresses that are allowed to authenticate (IEEE 802.11)
# with the AP. Optional VLAN ID can be assigned for clients based on the
# MAC address if dynamic VLANs (hostapd.conf dynamic_vlan option) are used.
